
[12:00:50] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[12:00:50] Disable I2C section
