
[11:44:26] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[11:44:26] Disable I2C section

[14:07:42] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[14:07:42] Disable I2C section

[14:16:50] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[14:16:50] Disable I2C section

[14:26:58] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[14:26:58] Disable I2C section

[14:32:40] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[14:32:40] Disable I2C section

[14:32:40] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x31, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x33, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x35, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x37, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x39, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3d, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3f, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x41, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x43, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x45, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x2e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x30, Length: 1, Value: 0x00 
[14:32:40] Disable I2C section

[14:33:15] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[14:33:15] Disable I2C section

[14:33:15] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x31, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x33, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x35, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x37, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x39, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3d, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3f, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x41, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x43, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x45, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x2e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x30, Length: 1, Value: 0x00 
[14:33:15] Disable I2C section

[14:36:29] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[14:36:29] Disable I2C section

[14:36:29] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x31, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x33, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x35, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x37, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x39, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3d, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3f, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x41, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x43, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x45, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x2e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x30, Length: 1, Value: 0x00 
[14:36:29] Disable I2C section

[15:01:40] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[15:01:40] Disable I2C section

[15:01:40] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x31, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x33, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x35, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x37, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x39, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3d, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3f, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x41, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x43, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x45, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x2e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x30, Length: 1, Value: 0x00 
[15:01:40] Disable I2C section

[17:43:28] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[17:43:28] Disable I2C section

[17:43:28] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x31, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x33, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x35, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x37, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x39, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3d, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3f, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x41, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x43, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x45, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x2e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x30, Length: 1, Value: 0x00 
[17:43:28] Disable I2C section

[17:45:53] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[17:45:53] Disable I2C section

[17:45:53] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x31, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x33, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x35, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x37, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x39, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3d, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3f, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x41, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x43, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x45, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x2e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x30, Length: 1, Value: 0x00 
[17:45:53] Disable I2C section

[17:46:30] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[17:46:30] Disable I2C section

[17:46:30] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x31, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x33, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x35, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x37, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x39, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3d, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3f, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x41, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x43, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x45, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x2e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x30, Length: 1, Value: 0x00 
[17:46:30] Disable I2C section

[17:48:47] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[17:48:47] Disable I2C section

[17:48:47] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x31, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x33, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x35, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x37, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x39, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3d, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3f, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x41, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x43, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x45, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x2e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x30, Length: 1, Value: 0x00 
[17:48:47] Disable I2C section
