
[14:32:54] Enable I2C section ( 0x53, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x70 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x80 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x12 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x03 48 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 C8 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x24 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0xC3 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x05 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x63 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 DC 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x4B 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x3D 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0xA2 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x48 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x14 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0xC0 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x7A 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x54 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0xD7 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x7F 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x1F 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0xF4 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x76 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x4C 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0xFF 
[14:32:54] Disable I2C section

[14:32:54] Enable I2C section ( 0x53, I2CRead )
(S) ReadThroughGRWM => Addr: 0x31, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x33, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x35, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x37, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x39, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3d, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3f, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x41, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x43, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x45, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x2e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2f, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x30, Length: 1, Value: 0x00 
[14:32:54] Disable I2C section

[14:32:58] Enable I2C section ( 0x53, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x70 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x80 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x12 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x03 48 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 C8 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x24 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0xC3 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x05 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x63 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 DC 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x4B 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x3D 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0xA2 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x48 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x14 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0xC0 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x7A 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x54 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0xD7 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x7F 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x1F 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0xF4 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x76 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x4C 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0xFF 
[14:32:58] Disable I2C section

[14:33:16] Enable I2C section ( 0x53, I2CWrite )
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) Write through GRWM => Addr: 0x12, Length: 1, Value: 0x40 
(S) Write through GRWM => Addr: 0x13, Length: 1, Value: 0x01 
[14:33:16] Disable I2C section

[14:33:18] Enable I2C section ( 0x53, I2CWrite )
(S) Write through GRWM => Addr: 0x13, Length: 1, Value: 0x81 
[14:33:18] Disable I2C section

[14:33:19] Enable I2C section ( 0x53, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x70 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x0E 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x80 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x10 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x12 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x03 48 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 C8 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x24 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0xC3 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x05 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x63 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 DC 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x4B 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x3D 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0xA2 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x48 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x81 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x14 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0xC0 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x7A 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x54 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0xD7 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x7F 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x1F 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0xF4 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x76 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x4C 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0xFF 
[14:33:19] Disable I2C section

[14:33:25] Enable I2C section ( 0x53, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x70 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x0E 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x80 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x12 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x03 48 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 C8 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x24 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0xC3 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x05 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x63 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 DC 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x4B 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x3D 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0xA2 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x48 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x81 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x14 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0xC0 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x7A 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x54 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0xD7 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x7F 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x1F 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0xF4 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x76 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x4C 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0xFF 
[14:33:25] Disable I2C section

[14:33:26] Enable I2C section ( 0x53, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x70 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x0E 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x80 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x12 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x03 48 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 C8 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x24 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0xC3 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x05 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x63 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 DC 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x4B 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x3D 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0xA2 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x48 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x81 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x14 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0xC0 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x7A 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x54 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0xD7 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x7F 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x1F 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0xF4 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x76 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x4C 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0xFF 
[14:33:26] Disable I2C section

[14:35:27] Enable I2C section ( 0x53, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x70 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x0E 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x80 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x12 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x03 48 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 C8 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x24 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0xC3 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x05 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x63 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 DC 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x4B 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x3D 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0xA2 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x48 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x81 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x14 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0xC0 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x7A 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x54 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0xD7 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x7F 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x1F 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0xF4 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x76 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x4C 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0xFF 
[14:35:27] Disable I2C section

[14:35:41] Enable I2C section ( 0x53, I2CWrite )
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 DC 
(S) Write through GRWM => Addr: 0x0b, Length: 2, Value: 0x01 40 
[14:35:41] Disable I2C section

[14:35:41] Enable I2C section ( 0x53, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x70 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x0E 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x80 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x12 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x03 48 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 C8 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x24 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0xC3 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x05 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x63 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x01 40 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x4B 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x3D 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0xA2 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x48 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x81 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x14 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0xC0 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x7A 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x54 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0xD7 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x7F 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x1F 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0xF4 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x76 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x4C 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0xFF 
[14:35:41] Disable I2C section

[14:35:42] Enable I2C section ( 0x53, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x70 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x0E 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x80 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x12 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x03 48 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 C8 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x24 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0xC3 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x05 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x63 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x01 40 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x4B 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x3D 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0xA2 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x48 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x40 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x81 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x14 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0xC0 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x7A 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x54 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0xD7 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x7F 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x1F 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0xF4 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x76 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x4C 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0xFF 
[14:35:42] Disable I2C section

[14:48:47] Enable I2C section ( 0x53, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x70 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x02 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x12 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x03 48 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 C8 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x24 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0xC3 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x05 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x63 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 DC 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x4B 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x3D 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0xA2 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x48 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x01 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x14 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0xC0 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x7A 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x54 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x01 2C 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0xD7 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x7F 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x1F 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0xFF 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0xF4 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x76 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x4C 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0xFF 
[14:48:48] Disable I2C section

[14:48:55] Enable I2C section ( 0x53, I2CWrite )
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) Write through GRWM => Addr: 0x12, Length: 1, Value: 0x40 
[14:48:55] Disable I2C section

[14:49:32] Enable I2C section ( 0x53, I2CWrite )
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 DC 
(S) Write through GRWM => Addr: 0x0b, Length: 2, Value: 0x01 40 
[14:49:32] Disable I2C section

[17:44:28] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x48, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x1f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x20, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x21, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x22, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x23, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x24, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x25, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x26, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x27, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x00, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x01, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x03, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x05, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x06, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x08, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x09, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x0d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x0f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x10, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x11, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x12, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x13, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x14, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x16, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x17, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x18, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x19, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x28, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x29, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2d, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x47, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x49, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4a, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4b, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4c, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x4e, Length: 1, Value: 0x00 
[17:44:28] Disable I2C section

[17:44:28] Enable I2C section ( 0xfe, I2CRead )
(S) ReadThroughGRWM => Addr: 0x31, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x33, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x35, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x37, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x39, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3b, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3d, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x3f, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x41, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x43, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x45, Length: 2, Value: 0x00 00 
(S) ReadThroughGRWM => Addr: 0x2e, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x2f, Length: 1, Value: 0x00 
(S) ReadThroughGRWM => Addr: 0x30, Length: 1, Value: 0x00 
[17:44:28] Disable I2C section
